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Two new products for CONTRAFLAM STRUCTURE family
More design variety for high-quality fire-resistant glass

A wide range of colour variations, more daylight and high transparency: with CONTRAFLAM STRUCTURE Elegance and CONTRAFLAM STRUCTURE Vibrance, Vetrotech Saint-Gobain is adding two more design highlights to its proven CONTRAFLAM STRUCTURE product family. The new products open up further design freedom in indoor and protected outdoor areas.

Slim, filigree, frameless, flush, durable: for twenty years CONTRAFLAM STRUCTURE has enabled the design of uncompromisingly safe rooms with the appearance of continuous, uninterrupted glass walls. The patented solution, which is highly valued by planners, architects and building owners, has been convincing in many configurations during this time. Now Vetrotech Saint-Gobain is continuing the success story of the first frameless, tempered fire-resistant glass with interlayer. With CONTRAFLAM STRUCTURE Elegance and CONTRAFLAM STRUCTURE Vibrance, the company is introducing two glasses that further extend the scope for design and thus offer even more possibilities for the development of individual and perfectly fitting solutions. 

Maximum daylight with minimum visual obstruction due to a very thin butt joint: With CONTRAFLAM STRUCTURE Elegance, it has been made possible to reduce the filigree silicone joint of CONTRAFLAM STRUCTURE by a further 10 mm. As a result, the glass has the thinnest line of sight of all "hardened" butt joint fire protection glazing and thus enables the design of light-flooded rooms with highly efficient fire protection. CONTRAFLAM STRUCTURE Elegance is suitable for interior applications and has the same robustness as the original. It is available in heights up to 3,210 mm and for fire resistance classes EI 30 and EI 60.

Design tone in tone or set contrasts: With CONTRAFLAM STRUCTURE Vibrance, fire-resistant glass can be colour-coordinated with the surroundings. The vertical edges painted on the back are available in practically any Pantone or RAL colour and can thus achieve a uniformly restrained effect or set invigorating accents with contrasting colours, depending on your wishes and concept. By choosing neutral or reserved colours, for example, the glass merges visually with the background, making it virtually disappear. Optical counterpoints can, in turn, be set by picking up colours from the surroundings and thus explicitly using the glass walls as design elements. 
CONTRAFLAM STRUCTURE Vibrance is robust, flexible and suitable for indoor use as well as for applications in protected outdoor areas. The glass is available in heights up to 3,800 mm for fire resistance classes EW 30/60 to EI 30/120 and can be combined with other features.

CONTRAFLAM STRUCTURE product family: the patented flush glazing

CONTRAFLAM STRUCTURE is a system made out of CONTRAFLAM EW30 to EI120 fire-rated glass, specially designed for use as a partition wall. Due to the special glazing with filigree, vertically arranged silicone joints, CONTRAFLAM STRUCTURE does not require vertical frame profiles. This creates aesthetically pleasing and open room solutions that allow natural daylight and outstanding sound insulation values, which were previously not possible in fire protection.

The room-high glasses of CONTRAFLAM STRUCTURE consist of thermally toughened single-pane safety glass (ESG) and interlayer layers in between. In the event of fire, these foam up and have a heat-insulating effect. The interlayer, which is based on nanotechnology, is inherently UV-resistant and is also characterized by its high light transmission. The excellent UV stability of the glass is at least 2.5 times higher than required by standards, making the glass extremely durable. Due to its design as hardened, laminated safety glass, CONTRAFLAM STRUCTURE has excellent impact resistance and is easy to handle, even with large pane dimensions.

All glasses in the Vetrotech product range can be combined with other features so that they cover the entire range of design and application areas. In addition, CONTRAFLAM STRUCTURE meets the requirements for the use of shatterproof materials in escape and traffic routes. The system can also be used in a wide variety of ways in wood, steel and aluminium profiles or in other frame constructions.
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About Vetrotech SAINT-GOBAIN International:
Vetrotech SAINT-GOBAIN International AG belongs to the SAINT-GOBAIN Group. Vetrotech specializes in the development, production and marketing of high-performance safety glass for the building sector and for shipping. The focus is on offering tailor-made multifunctional safety, comfort and design features for safe and seamless building integration. Customers benefit from the high level of consulting competence and know-how of Vetrotech's experts.

For Vetrotech, the safety of human life comes first: Vetrotech makes no compromises when it comes to protecting life and property. To this end, Vetrotech transforms the almost infinite potential of glass into high-performance solutions. Whatever the threat, Vetrotech uses its experience, ingenuity and know-how to make living spaces safe and permanently liveable for people.

Thanks to a wide range of fire-resistant, impact-resistant, attack-resistant, bulletproof, blast-resistant, pressure-resistant and even hurricane-proof high-security glass, Vetrotech develops innovative solutions that provide safety and comfort in all living spaces, even for the most demanding applications. Solutions that make no compromises in function or aesthetics, and that blend discreetly into the surrounding architecture, offering the user unobtrusive protection.

With seven production sites on three continents and around 1,000 employees worldwide, Vetrotech ensures that customers in more than 60 countries are reliably supplied via its regional sales offices spread across the globe. You can find more information about Vetrotech at www.vetrotech.com. Or follow us on Twitter (@Vetrotech_Int).

About SAINT-GOBAIN:
SAINT-GOBAIN develops, produces and distributes materials and solutions designed for the well-being of everyone and the future of all. These materials are found everywhere in our environment and in our daily lives: in buildings, transport, infrastructures and in numerous industrial applications. They provide comfort, performance and safety while meeting the requirements of sustainable construction, efficient use of resources and climate change. SAINT-GOBAIN is active in 67 countries and employs over 180,000 people. In the year 2018, a turnover of 41.7 billion euros was achieved. For more information about SAINT-GOBAIN, please visit www.saint-gobain.com or @saintgobain.
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